Cause:
- the determined number of pulses per revolution for the encoder is not plausible
Remedial action:
- check the friction wheel (traction, bearing, diameter)
- switch ZAdyn off and on again
- in case of permanent appearance: please contact ZIEHL-ABEGG customer service