Cause:
- the brake monitoring system has reacted during travel
Remedial action:
- check the correct functioning of the monitoring contacts
- check the brake activation and control
- check the supply voltage of the brakes