Cause:
- The state of the signals STO_A and STO_B was different for longer than 310 ms. The ZAdyn is locked by the internal hardware diagnosis.
Remedial action:
- check the activation and control of the STO inputs
- the error can only be reset by switching off the ZAdyn