XX    <-----------  Set country code. 
                    This language is active
                    after updating. XX = Language remains

*************************************************************
*
* file: default.txt
*
*************************************************************
* ZIEHL-ABEGG SE                           D-74653 Kuenzelsau
*                                       
*     FAX:   +49(0)7940-16-249          
*     EMail: drives-service@ziehl-abegg.com  
*                                       
*************************************************************
*                                       
*        ZAdyn4
*                                              
*************************************************************

Code  Language	Textfile

XX    old language remains
00    Deutsch   DE.TXT
01    English   GB.TXT
02    Tuerkce   TR.TXT
03    Nederland NL.TXT
04    Espanol   ES.TXT
05    Italiano  IT.TXT
06    Svenska   SV.TXT
07    Czech     CZ.TXT
08    Francais  FR.TXT
09    Polski    PL.TXT
10    Russki    RU.TXT


*** Additional Information **********************************


=============================================================
File location: root/4CX/UPDATE/0_TEXT/default.txt (0=ZERO!)
=============================================================

This file "default.txt" is analyzed from the ZAdyn 
software Version 3.28 (or greater).

Task: Automated loading and starting of the desired
      language after a software update.


3 languages are integrated in the controller ever since 
software version 3.28. German and English are permanently 
installed.

The third language can be loaded from the MMC to the internal 
ROM. During power failure, this language is stored 
permanently.

When an update is finished
the country code in the first line of this file 
(see above left) determines the choice of the third language.

After update and reboot, this language is automatically 
activated.

*** !!! Important !!! ***************************************
*
* The code must be entered in the first and second column 
* in the fist line!
*
* Example:
*
* 04 Right
*
* 4  False
*  4 False
*
* The remaining text can be freely changed.
*
*************************************************************

Special cases:
--------------

What happens if this file is missing?

   Spanish will be the third language.
   After restarting, English is enabled.


What happens when German 00 (or English 01) is chosen?

   Spanish will be the third language.
   After the restart German (or English) is enabled.


Tip: Parameterization in factory
--------------------------------

After the update remove the MMC.
If for example Spanish is active and the adjuster changes 
the parameter "LCD" to French, then the Spanish is deleted
from the internal ROM.
	

The Info menu 00 indicates the third language that is 
available.

Example:  "V3.28-29059ES" = Espanol.

This information is also available in the parameter 
and error lists.


Last Change: 20.07.2010


*** End *****************************************************





