Cause:
- at the digital input parameterized with the function "PFU_BR", the signal for temperature monitoring of the braking resistor disappears in the 2nd parameter set during travel
Remedial action:
- check the brake resistor for overheating
- check the wiring of thermal contact of BR
- switch ZAdyn off and on again