Cause:
- error in velocity mode: the heartbeat of the elevator controller is off or does not occur within the set time periods
- error in position mode: the heartbeat of the elevator controller and/or encoder is off or does not occur within the set time periods
Remedial action:
- check the CAN connections
- check the corresponding devices for correctly set heartbeats