Cause:
- the temperature in the area of the safety circuit STO exceeds 75 degrees Celsius
Remedial action:
- check the functioning of the cooling fans
- ensure an ambient temperature below 55 degrees Celsius
- switch ZAdyn off and on again